Samraksh eMote .NOW
ConfigureContinuousModeWithThresholding Method (ADCInternal)
Collapse All Expand All Language Filter: All Language Filter: Multiple Language Filter: Visual Basic Language Filter: Visual Basic (Declaration) Language Filter: Visual Basic (Usage) Language Filter: C# Language Filter: C++/CLI
Visual Basic (Declaration)
Visual Basic (Usage)
C#
C++/CLI

Samraksh.eMote.DotNow Namespace > ADCInternal Class : ConfigureContinuousModeWithThresholding Method

Configure continuous mode adc sampling with a threshold timestamp
Syntax

- Visual Basic
- C#
- C++/CLI

    'Declaration

    Public Shared Function ConfigureContinuousModeWithThresholding( _
       ByVal SampleBuff() As UShort, _
       ByVal channel As Integer, _
       ByVal NumSamples As UInteger, _
       ByVal SamplingTime As UInteger, _
       ByVal threshold As UInteger _
    ) As DeviceStatus

    'Usage

    Dim SampleBuff() As UShort
    Dim channel As Integer
    Dim NumSamples As UInteger
    Dim SamplingTime As UInteger
    Dim threshold As UInteger
    Dim value As DeviceStatus

    value = ADCInternal.ConfigureContinuousModeWithThresholding(SampleBuff, channel, NumSamples, SamplingTime, threshold)

    public static DeviceStatus ConfigureContinuousModeWithThresholding(
       ushort[] SampleBuff,
       int channel,
       uint NumSamples,
       uint SamplingTime,
       uint threshold
    )

    public:
    static DeviceStatus ConfigureContinuousModeWithThresholding(
       array<ushort>^ SampleBuff,
       int channel,
       uint NumSamples,
       uint SamplingTime,
       uint threshold
    )

#### Parameters

SampleBuff
channel
NumSamples
SamplingTime
threshold

Requirements

Target Platforms: eMote .NOW

See Also

#### Reference

ADCInternal Class
ADCInternal Members

Send Feedback