Samraksh eMote .NOW
Accelerometer.GRange Enumeration
Collapse All Expand All Language Filter: All Language Filter: Multiple Language Filter: Visual Basic Language Filter: Visual Basic (Declaration) Language Filter: Visual Basic (Usage) Language Filter: C# Language Filter: C++/CLI
Visual Basic (Declaration)
Visual Basic (Usage)
C#
C++/CLI

Samraksh.eMote.SensorBoard Namespace : Accelerometer.GRange Enumeration

Range of accelerometer
Syntax

- Visual Basic
- C#
- C++/CLI

    'Declaration

    Public Enum Accelerometer.GRange
       Inherits System.Enum

    'Usage

    Dim instance As Accelerometer.GRange

    public enum Accelerometer.GRange : System.Enum

    public enum class Accelerometer.GRange : public System.Enum

Members

Member | Description
--- | ---
EightG | 8 G range
FourG | 4 G range
SixteenG | 16 G range
TwoG | 2 G range

Remarks
"Range" refers to the range of values returned.

The user can choose the units in which the resulting data should be interpreted.

Lower G gives better precision but limited range of values.

Higher G gives less precision but larger range of values.

Hence a value of 13 for FourG would be 26 for TwoG.

Inheritance Hierarchy

System.Object
System.ValueType
System.Enum
Samraksh.eMote.SensorBoard.Accelerometer.GRange

Requirements

Target Platforms: eMote .NOW

See Also

#### Reference

Samraksh.eMote.SensorBoard Namespace

Send Feedback