Samraksh eMote .NOW
SetAddress Method (Radio_802_15_4_Base)
Collapse All Expand All Language Filter: All Language Filter: Multiple Language Filter: Visual Basic Language Filter: Visual Basic (Declaration) Language Filter: Visual Basic (Usage) Language Filter: C# Language Filter: C++/CLI
Visual Basic (Declaration)
Visual Basic (Usage)
C#
C++/CLI

Samraksh.eMote.Net.Radio Namespace > Radio_802_15_4_Base Class : SetAddress Method

Address of the device
Set the address of the device
Syntax

- Visual Basic
- C#
- C++/CLI

    'Declaration

    Public Function SetAddress( _
       ByVal address As UShort _
    ) As Boolean

    'Usage

    Dim instance As Radio_802_15_4_Base
    Dim address As UShort
    Dim value As Boolean

    value = instance.SetAddress(address)

    public bool SetAddress(
       ushort address
    )

    public:
    bool SetAddress(
       ushort address
    )

#### Parameters

address
  Address of the device

#### Return Value

Success / failure
Remarks
This is the address by which the device is known to the rest of the world. A return value of false can occur if another layer locks the address and prevents changes.
Requirements

Target Platforms: eMote .NOW

See Also

#### Reference

Radio_802_15_4_Base Class
Radio_802_15_4_Base Members

Send Feedback